2020.1:
 * Version 6.2 (Rev. 11)
 * General: Added security attribute

2019.2.2:
 * Version 6.2 (Rev. 10)
 * No changes

2019.2.1:
 * Version 6.2 (Rev. 10)
 * No changes

2019.2:
 * Version 6.2 (Rev. 10)
 * General: Updated the waivers for CDC
 * Revision change in one or more subcores

2019.1.3:
 * Version 6.2 (Rev. 9)
 * No changes

2019.1.2:
 * Version 6.2 (Rev. 9)
 * No changes

2019.1.1:
 * Version 6.2 (Rev. 9)
 * No changes

2019.1:
 * Version 6.2 (Rev. 9)
 * General: Updated the waivers for CDC
 * Revision change in one or more subcores

2018.3.1:
 * Version 6.2 (Rev. 8)
 * No changes

2018.3:
 * Version 6.2 (Rev. 8)
 * General: Supported devices and production status are now determined automatically, to simplify support for future devices

2018.2:
 * Version 6.2 (Rev. 7)
 * General: Added device support for virtexuplus58gf family

2018.1:
 * Version 6.2 (Rev. 6)
 * General: Updated ILA to handle XDC warnings

2017.4:
 * Version 6.2 (Rev. 5)
 * General: Updated ILA to handle XDC warnings

2017.3:
 * Version 6.2 (Rev. 4)
 * Added new virtexupluxHBM device support

2017.2:
 * Version 6.2 (Rev. 3)
 * Added new AZYNQUPLUS device support

2017.1:
 * Version 6.2 (Rev. 2)
 * Updated ILA and Debug Hub IPs to handle CDC warnings
 * Revision change in one or more subcores

2016.4:
 * Version 6.2 (Rev. 1)
 * Updated ILA and Debug Hub IPs to handle CDC warnings
 * Revision change in one or more subcores

2016.3:
 * Version 6.2
 * Updated DRC to set individual probe MU count value based on all_probe_same_mu_cnt parameter
 * Source HDL files are concatenated into a single file to speed up synthesis and simulation. No changes required by the user
 * Revision change in one or more subcores

2016.2:
 * Version 6.1 (Rev. 1)
 * Revision change in one or more subcores

2016.1:
 * Version 6.1
 * Updated the IP to support 2 Windows & 1 Sample count configuration
 * Number of comparator increased from 1 to 16 in basic mode and 4 to 16 in advanced mode
 * Updated probe data width register
 * Revision change in one or more subcores

2015.4.2:
 * Version 6.0 (Rev. 1)
 * No changes

2015.4.1:
 * Version 6.0 (Rev. 1)
 * No changes

2015.4:
 * Version 6.0 (Rev. 1)
 * No change
 * Revision change in one or more subcores

2015.3:
 * Version 6.0
 * Fixed Timing10 DRC violations in ILA IP.
 * IP revision number added to HDL module, library, and include file names, to support designs with both locked and upgraded IP instances
 * Revision change in one or more subcores

2015.2.1:
 * Version 5.1 (Rev. 1)
 * No changes

2015.2:
 * Version 5.1 (Rev. 1)
 * Updated IP XDC constraints to fix Partial False path scenario in ILA when operated in mulit clock domain
 * Updated IP XDC constraints to fix critical warnings in High Speed Design Debugging mode

2015.1:
 * Version 5.1
 * Fixed example design placer issue with pin location constraints for SVD packages

2014.4.1:
 * Version 5.0 (Rev. 2)
 * Updated example XDC pin location constraints for new devices

2014.4:
 * Version 5.0 (Rev. 1)
 * Encrypted source files are concatenated together to reduce the number of files and to reduce simulator compile time

2014.3:
 * Version 5.0
 * Added AXI4 Stream monitor support. New parameter option AXI4S added to C_SLOT_0_AXI_PROTOCOL
 * Four new user parameters added to support AXI4 Stream. These are C_SLOT_0_AXIS_TDATA_WIDTH, C_SLOT_0_AXIS_TID_WIDTH, C_SLOT_0_AXIS_TUSER_WIDTH, C_SLOT_0_AXIS_TID_WIDTH
 * Updated ILA IP to use new helper libraries (ltlib_v1_0 & xsdbs_v1_0)
 * Changed C_NNUM_MONITOR_SLOTS field to read only as ILA supported only interface in AXI mode

2014.2:
 * Version 4.0 (Rev. 1)
 * Fixed TIMING DRC violations, added ASYNC_REG property on the register which has double synchronizer for CDC paths
 * Fixed re-execution of First state when ila is used in advanced trigger mode
 * Reduced number of unused ports visible to users for AXI mode when AXI4LITE protocol is selected

2014.1:
 * Version 4.0
 * Updated the IP to support new DBG_HUB stitcher algorithm
 * Updated ILA AXI monitor feature to the IP
 * Internal device family name change, no functional changes

2013.4:
 * Version 3.0 (Rev. 1)
 * Kintex UltraScale Pre-Production support

2013.3:
 * Version 3.0
 * All ports changed to lower case
 * Added ILA Advanced Trigger Features

2013.2:
 * Version 2.1
 * Improved support for multiple instances
 * Added C_TRIGOUT_EN  parameter to support cross trigring
 * Added C_TRIGIN_EN  parameter to support cross trigring

2013.1:
 * Version 2.0
 * Native Vivado Release

(c) Copyright 2000 - 2020 Xilinx, Inc. All rights reserved.

This file contains confidential and proprietary information
of Xilinx, Inc. and is protected under U.S. and
international copyright and other intellectual property
laws.

DISCLAIMER
This disclaimer is not a license and does not grant any
rights to the materials distributed herewith. Except as
otherwise provided in a valid license issued to you by
Xilinx, and to the maximum extent permitted by applicable
law: (1) THESE MATERIALS ARE MADE AVAILABLE "AS IS" AND
WITH ALL FAULTS, AND XILINX HEREBY DISCLAIMS ALL WARRANTIES
AND CONDITIONS, EXPRESS, IMPLIED, OR STATUTORY, INCLUDING
BUT NOT LIMITED TO WARRANTIES OF MERCHANTABILITY, NON-
INFRINGEMENT, OR FITNESS FOR ANY PARTICULAR PURPOSE; and
(2) Xilinx shall not be liable (whether in contract or tort,
including negligence, or under any other theory of
liability) for any loss or damage of any kind or nature
related to, arising under or in connection with these
materials, including for any direct, or any indirect,
special, incidental, or consequential loss or damage
(including loss of data, profits, goodwill, or any type of
loss or damage suffered as a result of any action brought
by a third party) even if such damage or loss was
reasonably foreseeable or Xilinx had been advised of the
possibility of the same.

CRITICAL APPLICATIONS
Xilinx products are not designed or intended to be fail-
safe, or for use in any application requiring fail-safe
performance, such as life-support or safety devices or
systems, Class III medical devices, nuclear facilities,
applications related to the deployment of airbags, or any
other applications that could lead to death, personal
injury, or severe property or environmental damage
(individually and collectively, "Critical
Applications"). Customer assumes the sole risk and
liability of any use of Xilinx products in Critical
Applications, subject only to applicable laws and
regulations governing limitations on product liability.

THIS COPYRIGHT NOTICE AND DISCLAIMER MUST BE RETAINED AS
PART OF THIS FILE AT ALL TIMES.
